SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( CD_451019_bs
	comment ( Ppoollll, Jacek, Semora - verze 1.0 )
	comment ( Uprava svetel pro MSTS Bin 1.6 - Miran )
        Comment (verze ladeni 20-11-2006 - dle norem Ppoollll nastavil Semora) 
	Type ( Engine )
	WagonShape ( CD_451019_bs.s ) 
	Size ( 3.0m 5.55m 24.40m )
	CentreOfGravity ( 0m 1.5m 0m )
	Mass ( 65t )
	WheelRadius ( 0.5m )
	InertiaTensor ( Box ( 3.1m 5.55m 24.40m ))
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 2e6N/m/s )
			Break ( 1.1e8N 5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 2e6N/m/s )
			Break ( 1.1e8N 5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Adheasion ( 0.18 0.4 2 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*65t )
	DerailBufferForce ( 350kN )
	NumWheels ( 4 )
	Friction (
		930.3N/m/s  -0.1  1.0mph 8.880N/m/s  1.950
		5.1N/rad/s  1  -1rad/s  0  1
	)
	AntiSlip ()

	BrakeEquipmentType ( "handbrake, graduated_release_triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType ( "Air_single_pipe" )

	MaxBrakeForce ( 50kN )
	MaxHandbrakeForce ( 7kN )
	NumberOfHandbrakeLeverSteps ( 100 )
	EmergencyBrakeResMaxPressure ( 73 )
	EmergencyResCapacity ( 14 )
	EmergencyResChargingRate ( 10 ) 
	TripleValveRatio ( 2.48 )
	MaxReleaseRate ( 4.2 )
	MaxApplicationRate ( 5 )
	MaxAuxilaryChargingRate ( 5 )
	BrakeCylinderPressureForMaxBrakeBrakeForce ( 60 )

	PassengerCapacity ( 60.0 )

	Lights ( 10
		Light (
			comment ( Svetelny kuzel pred lokomotivou )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
			)
			Cycle ( 0 )
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( ffffeba4 )
					Position ( 0.0 3.5 18 )
					Transition ( 0 )
					Radius ( 400.0 )
					Angle ( 15.0 )
				)
			)
		)
		Light (
			comment ( Horni predni svetlomet plne )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( fffff3d2 )
					Position ( 0.0 3.45 11.94 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
			)
		)
		Light (
			comment ( Leve predni pozicni off )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 0 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFF0E3B5 )
					Position ( -1.1 1.55 11.77 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Prave predni pozicni off )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 0 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFF0E3B5 )
					Position ( 1.1 1.55 11.77 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Leve predni pozicni off reverse )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 4 )
				Control ( 0 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFF0E3B5 )
					Position ( -1.1 1.55 11.77 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Prave predni pozicni off reverse)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 4 )
				Control ( 0 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFF0E3B5 )
					Position ( 1.1 1.55 11.77 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Levé prední cervene)
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 0 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( 1.1 1.55 11.77 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Pravé predni cervene)
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 0 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( -1.1 1.55 11.77 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Levé přední poziční off - posun )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFF0E3B5 )
					Position ( -1.1 1.55 11.77 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Pravé přední poziční off - posun )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFF0E3B5 )
					Position ( 1.1 1.55 11.77 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
   	)
	Sound ( "../../common.snd/sndelok/451eng.sms" )
)
Engine ( CD_451019_bs
	Wagon ( CD_451019_bs )
	Type ( Electric )
	MaxPower ( 660kW )
	MaxForce ( 70kN )
	MaxContinuousForce ( 60kN )
	MaxVelocity ( 100km/h )
	MaxCurrent ( 300A )
	WheelRadius ( 0.5m )
	Sanding ( 40km/h )
	NumWheels ( 4 )

	AirBrakesAirCompressorPowerRating ( 1.5 )
	AirBrakesMainMinResAirPressure ( 56 )
	AirBrakesMainMaxAirPressure ( 117 )
	AirBrakesMainResVolume ( 9.5 )
	AirBrakesAirCompressorWattage ( 20000 )
	AirBrakesCompressorRestartPressure ( 87 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 0.5 )
	AirBrakesHasLowPressureTest ( 0 )
	AirBrakesIsCompressorElectricOrMechanical ( 0 )

	EngineBrakesControllerMinPressureReduction ( 3.0 )
	EngineBrakesControllerMaxPressureDropInNormalApplication ( 22.5 )
	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesProportionalBrakeLag ( 0.81 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 20 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerFullServicePressureDrop ( 40 )

	TrainBrakesControllerMinPressureReduction ( 3.0 )
	TrainBrakesControllerMaxPressureDropInNormalApplication ( 22.5 )
	TrainBrakesControllerMinContinuousService ( 20 )
	TrainBrakesControllerMaxApplicationRate( 1.9 )
	TrainBrakesControllerMaxReleaseRate( 2 )
	TrainBrakesControllerMaxQuickReleaseRate ( 5 )
	TrainBrakesControllerEmergencyApplicationRate ( 15 )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 73 )
	TrainPipeLeakRate ( 0.1 )
	TrainBrakesControllerFullServicePressureDrop ( 22.5 )

	DynamicBrakesMinUsableSpeed ( 12.5 )
        DynamicBrakesCutInSpeed ( 13 )
	DynamicBrakesFadingSpeed ( 42 )
	DynamicBrakesMaximumEffectiveSpeed ( 54 )
	DynamicBrakesMaximumForce ( 50kN )
	DynamicBrakesResistorCurrentLimit ( 300 )
	DynamicBrakesMaxAirBrakePressure ( 50 )
	DynamicBrakesDelayTimeBeforeEngaging ( 1 )
	DynamicBrakesMaximumSpeedForFadeOut ( 110 )
	DynamicBrakesEffectAtMaximumFadeOut ( 0 )
	DynamicBrakesHigherSpeedCurveExponent ( 1 )
	DynamicBrakesLowerSpeedCurveExponent ( 3 )
	DynamicBrakesNumberOfControllerNotches ( 3 )
	DynamicBrakeHasAutoBailOff ( 0 )
 
	BrakesEngineBrakeType ( "Air_single_pipe"  )
	BrakesTrainBrakeType ( "Air_single_pipe" )
	BrakesEngineControllers ( "Independent, Train, Dynamic" )

	CabView ( "..\\..\\common.cab\\cab451\\451.cvf" )
	Headout ( 1.75 2.6 10.3 )

	EngineBrakesControllerDirectControlExponent ( 1 )

	DoesHornTriggerBell ( 0 )

EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 20 )
		MonitoringDeviceAlarmTimeLimit ( 10 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	OverspeedMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 5 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 65.1 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 )
		MonitoringDeviceDoesSuppressionReset ( 0 )
		MonitoringDeviceTriggerOnOverspeed ( 65.2 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 0 )
	)
	EngineControllers (
		Throttle ( 0 1 0.01 0
			NumNotches ( 5
				Notch ( 0     0 Dummy )
				Notch ( 0.44  0 Dummy )
				Notch ( 0.65  0 Dummy )
				Notch ( 0.85  0 Dummy )
				Notch ( 1.00  0 Dummy )
			)
		)
		Brake_Engine ( 0 1 0.1 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)
		Brake_Train ( 0 1 0.05 0.85
			NumNotches ( 8
				Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.21 0 TrainBrakesControllerHoldLappedStart )
				Notch ( 0.33 0 TrainBrakesControllerMinimalReductionStart )
				Notch ( 0.34 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
				Notch ( 0.76 0 TrainBrakesControllerSuppressionStart )
				Notch ( 0.85 0 TrainBrakesControllerContinuousServiceStart )
				Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
			)
		)
		Brake_Hand ( 0 1 0.05 0 
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)
		Brake_Dynamic ( 0 1 0 0 
			NumNotches ( 3
				Notch ( 0.0 0 Dummy )
				Notch ( 0.3 0 Dummy )
				Notch ( 1.0 0 Dummy )
			)
		)
		Combined_Control ( 0 2 1 1 throttle dynamic )
		DirControl ( -1 0 1 1 )
		EmergencyStopToggle ( 0 1 0 )
		AWS ( 0 1 0 )
		Sanding ( 0 1 0 )
		Horn ( 0 1 0 )
		BellToggle ( 0 1 0 )
		Vigilance ( 0 1 0 )
		PantographToggle1 ( 0 1 0 )
		Headlights ( 0 0.25 1 0 )
		Wipers ( 0 1 0 )
		BailOffButton ( 0 1 0 )
	)
	Name ( "CD 451.019-4 bs" )
	Description (
		"Elektricka jednotka CD rady 451.\n"+
		"Napetova soustava 3kV ss.\n\n"+
		"Delka jednotky (2+2 vozy): 95890mm\n\n"+
		"Prumer hnacich kol: 1000 mm\n\n"+
		"Celkova hmotnost: 182,4 t\n\n"+
		"Trvaly vykon: 1320 kW\n\n"+
		"Max. rychlost 100 km/h\n\n"+
		"Vyroba Moravskoslezska vagonka Studenka 1964-68\n\n"
	)
	EngineOperatingProcedures (
		"Tato verze modelu je urcená na celo druhé soupravy.\n"+"
		"V pripade rozpojeni soupravy lze s touto jednotkou\n"+
		"jet v cele vlaku"
	)
	Sound ( "..\\..\\common.snd\\sndelok\\451cab.sms" )
)