SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( CD_451019
	comment ( Ppoollll, Jacek, Semora - verze 1.0 )
	comment ( Uprava svetel pro MSTS Bin - Miran )
        Comment (verze ladeni 20-11-2006 - dle norem Ppoollll nastavil Semora)
	Type ( Engine )
	WagonShape ( CD_451019.s ) 
	Size ( 3.0m 5.55m 24.40m )
	CentreOfGravity ( 0m 1.5m 0m )
	Mass ( 65t )
	WheelRadius ( 0.5m )
	InertiaTensor ( Box ( 3.1m 5.55m 24.40m ))
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 2e6N/m/s )
			Break ( 1.1e8N 5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 2e6N/m/s )
			Break ( 1.1e8N 5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Adheasion ( 0.18 0.4 2 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*65t )
	DerailBufferForce ( 350kN )
	NumWheels ( 4 )
	Friction (
		930.3N/m/s  -0.1  1.0mph 8.880N/m/s  1.950
		5.1N/rad/s  1  -1rad/s  0  1
	)
	AntiSlip ()

	BrakeEquipmentType ( "handbrake, graduated_release_triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType ( "Air_single_pipe" )

	MaxBrakeForce ( 50kN )
	MaxHandbrakeForce ( 7kN )
	NumberOfHandbrakeLeverSteps ( 100 )
	EmergencyBrakeResMaxPressure ( 73 )
	EmergencyResCapacity ( 14 )
	EmergencyResChargingRate ( 10 ) 
	TripleValveRatio ( 2.48 )
	MaxReleaseRate ( 4.2 )
	MaxApplicationRate ( 5 )
	MaxAuxilaryChargingRate ( 5 )
	BrakeCylinderPressureForMaxBrakeBrakeForce ( 60 )

	PassengerCapacity ( 60.0 )
	Inside (
		PassengerCabinFile ( CD_451019.s )
		PassengerCabinHeadPos ( -1.6 3.0 10.5 )
		RotationLimit ( 45.0 180.0 0.0 )
		StartDirection ( 0 -10 0 )
		Sound ( "..\\..\\common.snd\\sndelok\\451eng.sms" )
	)

	Lights ( 10
		Light (
			comment ( Svetelny kuzel pred lokomotivou )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
			)
			Cycle ( 0 )
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( ffffeba4 )
					Position ( 0.0 3.5 18 )
					Transition ( 0 )
					Radius ( 400.0 )
					Angle ( 15.0 )
				)
			)
		)
		Light (
			comment ( Horni predni svetlomet plne )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( fffff3d2 )
					Position ( 0.0 3.45 11.94 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
			)
		)
		Light (
			comment ( Leve predni pozicni bile )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 0 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFF0E3B5 )
					Position ( -1.1 1.55 11.77 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Prave predni pozicni bile )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 0 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFF0E3B5 )
					Position ( 1.1 1.55 11.77 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Leve predni pozicni bile reverse )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 4 )
				Control ( 0 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFF0E3B5 )
					Position ( -1.1 1.55 11.77 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Prave predni pozicni bile reverse)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 4 )
				Control ( 0 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFF0E3B5 )
					Position ( 1.1 1.55 11.77 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Levé prední cervene)
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 0 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( 1.1 1.55 11.77 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Pravé predni cervene)
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 0 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( -1.1 1.55 11.77 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Levé přední poziční off - posun )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFF0E3B5 )
					Position ( -1.1 1.55 11.77 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Pravé přední poziční off - posun )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFF0E3B5 )
					Position ( 1.1 1.55 11.77 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
	)
	Sound ( "..\\..\\common.snd\\sndelok\\451eng.sms" )
)
Engine ( CD_451019
	Wagon ( CD_451019 )
	Type ( Electric )
	MaxPower ( 660kW )
	MaxForce ( 70kN )
	MaxContinuousForce ( 60kN )
	MaxVelocity ( 100km/h )
	MaxCurrent ( 300A )
	WheelRadius ( 0.5m )
	Sanding ( 40km/h )
	NumWheels ( 4 )

	AirBrakesAirCompressorPowerRating ( 1.5 )
	AirBrakesMainMinResAirPressure ( 56 )
	AirBrakesMainMaxAirPressure ( 117 )
	AirBrakesMainResVolume ( 9.5 )
	AirBrakesAirCompressorWattage ( 20000 )
	AirBrakesCompressorRestartPressure ( 87 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 0.5 )
	AirBrakesHasLowPressureTest ( 0 )
	AirBrakesIsCompressorElectricOrMechanical ( 0 )

	EngineBrakesControllerMinPressureReduction ( 3.0 )
	EngineBrakesControllerMaxPressureDropInNormalApplication ( 22.5 )
	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesProportionalBrakeLag ( 0.81 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 20 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerFullServicePressureDrop ( 40 )

	TrainBrakesControllerMinPressureReduction ( 3.0 )
	TrainBrakesControllerMaxPressureDropInNormalApplication ( 22.5 )
	TrainBrakesControllerMinContinuousService ( 20 )
	TrainBrakesControllerMaxApplicationRate( 1.9 )
	TrainBrakesControllerMaxReleaseRate( 2 )
	TrainBrakesControllerMaxQuickReleaseRate ( 5 )
	TrainBrakesControllerEmergencyApplicationRate ( 15 )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 73 )
	TrainPipeLeakRate ( 0.1 )
	TrainBrakesControllerFullServicePressureDrop ( 22.5 )

	DynamicBrakesMinUsableSpeed ( 12.5 )
        DynamicBrakesCutInSpeed ( 13 )
	DynamicBrakesFadingSpeed ( 42 )
	DynamicBrakesMaximumEffectiveSpeed ( 54 )
	DynamicBrakesMaximumForce ( 50kN )
	DynamicBrakesResistorCurrentLimit ( 300 )
	DynamicBrakesMaxAirBrakePressure ( 50 )
	DynamicBrakesDelayTimeBeforeEngaging ( 1 )
	DynamicBrakesMaximumSpeedForFadeOut ( 110 )
	DynamicBrakesEffectAtMaximumFadeOut ( 0 )
	DynamicBrakesHigherSpeedCurveExponent ( 1 )
	DynamicBrakesLowerSpeedCurveExponent ( 3 )
	DynamicBrakesNumberOfControllerNotches ( 3 )
	DynamicBrakeHasAutoBailOff ( 0 )
 
	BrakesEngineBrakeType ( "Air_single_pipe"  )
	BrakesTrainBrakeType ( "Air_single_pipe" )
	BrakesEngineControllers ( "Independent, Train, Dynamic" )

	CabView ( "..\\..\\common.cab\\cab451\\451.cvf" )
	Headout ( 1.75 2.6 10.3 )

	EngineBrakesControllerDirectControlExponent ( 1 )

	DoesHornTriggerBell ( 0 )

EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 20 )
		MonitoringDeviceAlarmTimeLimit ( 10 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	OverspeedMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 5 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 65.1 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 )
		MonitoringDeviceDoesSuppressionReset ( 0 )
		MonitoringDeviceTriggerOnOverspeed ( 65.2 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 0 )
	)

	EngineControllers (
		Throttle ( 0 1 0.01 0
			NumNotches ( 5
				Notch ( 0     0 Dummy )
				Notch ( 0.44  0 Dummy )
				Notch ( 0.65  0 Dummy )
				Notch ( 0.85  0 Dummy )
				Notch ( 1.00  0 Dummy )
			)
		)
		Brake_Engine ( 0 1 0.1 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)
		Brake_Train ( 0 1 0.05 0.85
			NumNotches ( 8
				Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.21 0 TrainBrakesControllerHoldLappedStart )
				Notch ( 0.33 0 TrainBrakesControllerMinimalReductionStart )
				Notch ( 0.34 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
				Notch ( 0.76 0 TrainBrakesControllerSuppressionStart )
				Notch ( 0.85 0 TrainBrakesControllerContinuousServiceStart )
				Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
			)
		)
		Brake_Hand ( 0 1 0.05 0 
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)
		Brake_Dynamic ( 0 1 0 0 
			NumNotches ( 3
				Notch ( 0.0 0 Dummy )
				Notch ( 0.3 0 Dummy )
				Notch ( 1.0 0 Dummy )
			)
		)
		Combined_Control ( 0 2 1 1 throttle dynamic )
		DirControl ( -1 0 1 1 )
		EmergencyStopToggle ( 0 1 0 )
		AWS ( 0 1 0 )
		Sanding ( 0 1 0 )
		Horn ( 0 1 0 )
		BellToggle ( 0 1 0 )
		Vigilance ( 0 1 0 )
		PantographToggle1 ( 0 1 0 )
		Headlights ( 0 0.25 1 0 )
		Wipers ( 0 1 0 )
		BailOffButton ( 0 1 0 )
	)
	Name ( "CD 451.019-4" )
	Description (
		"Elektricka jednotka CD rady 451.\n"+
		"Napetova soustava 3kV ss.\n\n"+
		"Delka jednotky (2+2 vozy): 95890mm\n\n"+
		"Prumer hnacich kol: 1000 mm\n\n"+
		"Celkova hmotnost: 182,4 t\n\n"+
		"Trvaly vykon: 1320 kW\n\n"+
		"Max. rychlost 100 km/h\n\n"+
		"Vyroba Moravskoslezska vagonka Studenka 1964-68\n\n"
	)
	EngineOperatingProcedures (
		"Jak se rozjet\n"+
		"1.	Uz mate zvednuty pantograf. (Pokud z nejakeho duvodu zvednuty neni, stisknete klavesu P pro jeho zvednuti.)\n"+
		"2.	Stisknete W na prestaveni reverzniho kontoleru do polohy 'vpred'.\n"+
		"3.	Stisknete a drzte ; pro odbrzdeni vlakove brzdy.\n"+
		" (4. Stisknete a drzte [ pro odbrzdeni lokomotivni brzdy.)\n"+
		"5.	Pridavejte jizdni stupne stiskem D, dokud vlak nedosahne pozadovane rychlosti. Pozor na prokluz! (Zelena kontrolka prokluzu na pulte loko nebo F5 zobrazi jizdni udaje.)\n\n"+
		"Jak zpomalit\n"+
		"1.	Stisknete A pro ubrani jizdnich stupnu ( postupne az na 0 ).\n"+
		"2.	Drzte stisknute i nadale A pro zarazeni 1 neboo 2 stupne EDB.\n"+
		" (Pozn.: Tato brzda je ucinna do 30 km/h. Pri nizsich rychlostech je nutne brzdit prubeznou brzdou.)\n\n"+
		"3.	Jestlize je to nutne tak pouzijte vzduchove vlakove brzdy pro postupne rychlejsi snizovani rychlosti.\n\n"+
		"Jak pouzit vlakovou brzdu\n"+
		"1.	Stisknete a drzte ' a dosahnete pozadovaneho brzdneho tlaku (0-100%).\n\n"+
		"Jak odbrzdit vlakovou brzdu\n"+
		"1.	Stisknete a drzte ; az presunete rukojet brzdy do polohy JiZDA.\n\n"+
		"Jak pouzit lokomotvni brzdu\n"+
		"1.	Stisknete a drzte ] pro zabrzdeni lokomotivni brzdy (0-100%).\n\n"+
		"Jak odbrzdit lokomotivni brzdu\n"+
		"1.	Stisknete a drzte [ pro odbrzdeni lokomotivni brzdy (0-100%).\n\n"+
		"Jak pouzit zachrannou brzdu\n"+
		"1.	Stisknete BACKSPACE pro aktivaci zachrane brzdy.\n"+
		"2.	Stisknete a drzte A pro ubrani jizdnich stupnu na 0.\n\n"+
		"Jak zrusit zachrannou brzdu\n"+
		"1.	Pockejte na uplne zastaveni vlaku.\n"+
		"2.	Stisknete Z pro odblokovani ovladani lokomotivy.\n"+
		"3.	Stisknete ; a [ pro odbrzdeni brzdnych systemu.\n"+
		" (Pozn.: Je-li rychlobrzda zavedena sama (pri prekroceni rychlosti nebo neobslouzeni zivaka), je po zastaveni nutno pockat 90s. Drive nelze odbrzdit).\n\n"+
		"Vystup a nastup cestujicich\n"+
		"1.	Zastavte ve stanici.\n"+
		"2.	Stisknete ENTER pro zahajeni vystupu a nastupu cestujicich.\n"+
		"3.	Pockejte na signal k odjezdu.\n"+
		"TIP: Pro zobrazeni casu prijezdu a odjezdu u teto a nasledujici stanice pouzijte klavesu F10.\n\n"+
		"Jak zmenit smer\n"+
		"1.	Zastavte vlak.\n"+
		"2.	Presunte paku reverzniho kontroleru do polohy vzad dvojitym stiskem S (nebo vpred W).\n"+
		"3.	Odbrzdete brzdy stiskem ; ( pripadne [ ).\n"+
		"4.	Pridavejte jizdni stupne stiskem D .\n\n"+
		"Jak pripojit vagony/lokomotivy:\n"+
		"1.	Najedte pomalu na soupravu (optimalni rychlost 1 km/h).\n"+
		"Tip: Pro zobrazeni pohledu na sprahlo stisknete klavesu 6.\n"+
		"2.	Stisknete F9 pro otevreni okna se seznamem lokomotiv a vagonu ve vlaku.\n"+
		"3.	Jestlize je ikona vozu cervena, je zatazena rucni brzda. Dvojtukem mysi na voze uvolnite/zatahne rucni brzdu.\n"+
		"4.	Zavrete okno sestaveni vlaku stiskem F9.\n"+
		"5.	Pockejte az odbrzdite pripojene vozy.\n\n"+
		"Odpojeni vozu nebo lokomotivy\n"+
		"POZOR! Melo by se provadet jen tehdy, pokud VLAK STOJi!\n"+
		"1.	Otevrete okno sestavy vlaku F9.\n"+
		"2.	Poklepejte 2x na ikonu vozu, ktery se ma odpojit, pokud chcete, aby mel vuz zatazenou rucni brzdu.\n"+
		"3.	Poklepejte mysi 2x na ikonu spoje, kde ma byt vlak rozdelen.\n"+
		"4.	Pomalu se rozjedte smerem od odpojene casti vlaku.\n"+
		" (Pozn.: V nekterych pripadech pri rychlejsim odjezdu dojde k opetovnemu spojeni sprahel. Pokud se toto stane tak soupravu opet rozpojte a velmi pomalu odjizdejte az do vzdalenosti jednoho prazce. Pak jiz muzete zacit zrychlovat.)\n"+
		"5.	Zavrete okno sestaveni vlaku stiskem F9.\n\n"+
		"DULEZITE UPOZORNENI\n"+
		"Souprava je jako celek v realu nerozpojitelna! Rozpojit ji lze jen v dilnach! Spojovat a rozpojovat lze pouze jednotlive soupravy mezi sebou. Pro pripojeni za lokomotivu se sroubovkou potrebujete pouzit prechodove sprahlo!\n"
	)
	Sound ( "..\\..\\common.snd\\sndelok\\451cab.sms" )
)